/\*\*/int redPin=11; //set red LED pin to 11int greenPin=10; //set green LED pin to 10void setup() { serial.begin (9600); //turn on serial portpinMode(greenpin, OUTPUT); //set green pin to be an outout 3pinMode(redpin, OUTPUT); //set red pin to be an outout }void loop() { digitalWrite(redpin,0); //turn off red pin delay(1000) digitalWrite(greenpin,0); //turn off green pin delay(1000) }

I FAILED BUT ITS OKAY ☺